NBS PLUS MANUFACTURER’S PRODUCT PAGE

|  |  |  |
| --- | --- | --- |
| Manufacturer: | Procter Contracts | TelescopicGates_Thmb |
| Product name: | Telescopic Gates |

[Jump to instructions](#Instructions)

Product summary: (a one sentence product description used to differentiate between similar products)

|  |
| --- |
| Steel telescopic gates. |

Product general description:

|  |
| --- |
| A telescopic gate has the advantage that it takes up less space compared to a tracked or cantilevered sliding gate when in the open position. This therefore makes it ideal for a site where space is restricted either side of an entrance, but where the entrance itself is relatively wide - a single telescopic gate can be used for an opening of up to 14 m, and a pair of gates for an opening of twice that size.  Matching pedestrian gate, automation and access controls available including CE marked safety equipment, consult manufacturers for details.  Applications:   * Warehousing. * Secure sites. * Utilities. * Airports. * Retail. * Industrial units. |

Product specification clause

Product reference:

|  |
| --- |
| Telescopic Gates SG-TG-002 |

Product properties:

|  |
| --- |
| * Colour/ Finish:   Polyester powder coated, RAL - Insert colour requirements.   * Infill:   Decorative infill panels  Steel balustrade  Timber cladding  Welded mesh |

End of product specification clause

As standard: (use this box to describe the features of the product that are provided as standard)

|  |
| --- |
| Height:  1.8–2.4 m. |

Options: (use this box to describe the features of the product that are optional)

|  |
| --- |
| Colour/ Finish:  Hot dip galvanized to BS EN ISO 1461:2009 and polyester coated to a range of RAL colours.  Infill:  A range of options including bespoke designs are available, consult manufacturer for details. |

Approvals: (use this box to list any third party product approvals, e.g. Kitemark and British Board of Agrément certificates)

|  |
| --- |
| No approvals |

<>

Product literature:

RPS ID: COL642008

Page number:

RPS ID: COL108683

Page number:

Manufacturer notes [not for publication]:

|  |
| --- |
|  |

Procter Contracts contact details:

Email: [Enquiries@proctercontracts.co.uk](mailto:Enquiries@proctercontracts.co.uk)

Telephone: 0808 2566 638

Address: 11 Pant Glas Est

Bedwas

Caerphilly

CF83 8XD

**Key:**

Within the "Product Specification Clause" section, the following notation is used:

[-] This is an empty insert, into which a specifier can enter their own requirements (e.g. colour or size).

[d] The value below this notation is the default value for a property, meaning that is selected automatically for the specifier.

[And] More than one item from the values below this notation may be selected by the specifier.